For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear floor console cupholder bezel assembly. Refer to Rear Floor Console Cup Holder Bezel Replacement.
2. Remove the rear floor console cupholder trim upper panel assembly. Refer to Rear Floor Console Cup Holder Trim Upper Panel Replacement.
3. Remove the rear floor console latch cover. Refer to Rear Floor Console Latch Cover Replacement.

1 | Rear Floor Console Front Trim Upper Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Floor Console Front Trim Upper Panel Assembly

#### Procedure

Use a flat-bladed plastic trim tool in order to release the clips securing the trim panel to the console assembly.