For 1990-2009 cars

## Rear Seat Cushion Frame Replacement With 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement.
3. Remove the rear seat latch cables. Refer to Rear Seat Latch Cable Replacement - Inboard or Rear Seat Latch Cable Replacement - Outboard.

1 | Rear Seat Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 28 N·m (21 lb ft)
2 | Rear Seat Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
3 | Rear Seat Cushion Frame Assembly

## Rear Seat Cushion Frame Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement.
3. Remove the rear seat latch cables. Refer to Rear Seat Latch Cable Replacement - Inboard or Rear Seat Latch Cable Replacement - Outboard.

1 | Rear Seat Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 28 N·m (21 lb ft)
2 | Rear Seat Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
3 | Rear Seat Cushion Frame Assembly