For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Hoist the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Steering Gear Valve Solenoid Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Steering Gear Valve Solenoid

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Transfer or replace any O-ring seals as needed.