For 1990-2009 cars

## Headlamp Replacement Traverse with TVP

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Fender Brace Bolt to Headlamp Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Headlamp Bolt Tighten 6 N·m (53 lb in)
3 | Headlamp Horizontal and Vertical Adjusting Cam Nut Bolt (Qty: 2)

#### Procedure

1. Set the cam adjusting nuts to the nominal setting of 6 turns off fully seated prior to installing the new headlamp assembly.
2. Check the front bumper fascia to headlamp finish fit and adjust the cam nuts accordingly to achieve an even fit.

4 | Headlamp Assembly Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

1. Gently pull forward the headlamp assembly.
2. Disconnect the forward lamp harness electrical connector from the headlamp assembly electrical connector.
3. Remove the headlamp from vehicle.
4. Transfer the headlamp electrical harness with bulb sockets as needed.

## Headlamp Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Headlamp Screws (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Fender Brace Screw to Headlamp Tighten 2 N·m (18 lb in)
3 | Headlamp Horizontal and Vertical Adjustment Nuts (Qty: 2)

#### Procedure

1. Set the cam adjusting nuts to the nominal setting of 6 turns off fully seated prior to installing the new headlamp assembly.
2. Check the front bumper fascia to headlamp finish fit and adjust the cam nuts accordingly to achieve an even fit.

4 | Headlamp Vertical Adjusting Bolt Bushing
5 | Headlamp Assembly

#### Procedure

1. Gently pull forward the headlamp assembly.
2. Disconnect the forward lamp harness from the headlamp assembly electrical connector.
3. Remove the headlamp from vehicle.

## Headlamp Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Headlamp Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Fender Brace Bolt to Headlamp Tighten 2 N·m (18 lb in)
3 | Headlamp Horizontal and Vertical Adjustment Nuts (Qty: 2)

#### Procedure

1. Set the cam adjusting nuts to the nominal setting of 6 turns off fully seated prior to installing the new assembly.
2. Check the front bumper fascia to headlamp finish fit and adjust the cam nuts accordingly to achieve an even fit.

4 | Headlamp Vertical Adjusting Bolt Bushing
5 | Headlamp Assembly

#### Procedure

1. Gently pull forward the headlamp assembly.
2. Disconnect the forward lamp harness from the headlamp assembly electrical connector.
3. Remove the headlamp from vehicle.

## Headlamp Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Headlamp Assembly Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tip Tighten the fasteners in sequence as shown. Tighten
6 N·m (53 lb in)

2 | Headlamp Assembly Nut Tighten 6 N·m (53 lb in)
3 | Headlamp Assembly

#### Procedure

Pull outward on the housing in order to disconnect the electrical connection at the lower rear edge of the lamp.

4 | Electrical Harness Connector

#### Procedure

Disconnect the electrical connector from the headlamp assembly.