For 1990-2009 cars

Important: The internal components of the torque tube assembly are not serviced separately. Replace the tube and internal components as an assembly.

1. Check the torque tube for the following conditions:

• | Damage to the driver flange

• | Cracks or dents on the exterior of the torque tube

• | Operation of all bearings

• | Machine surfaces for abnormal wear

2. If any of the above conditions are found to be present, replace the torque tube assembly.