For 1990-2009 cars

## Liftgate Applique Replacement Acadia

Callout | Component Name
--- | ---

#### Procedure

Remove the rear window wiper motor. Refer to Rear Window Wiper Motor Replacement.

1 | Center Applique Nuts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Center Applique Integral Clips

#### Procedure

Install the applique to the liftgate panel first by securing the integral clips.

3 | License Plate Lamp Electrical Connector

#### Procedure

Transfer the license plate lamp sockets and electrical harness to the new applique panel.

4 | Liftgate Center Applique

## Liftgate Applique Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Disconnect the rear liftgate applique electrical connector from the rear body harness.

1 | Liftgate Applique Nuts (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Liftgate Applique Electrical Harness and Grommet
4 | Liftgate Applique Assembly

#### Procedure

1. Disconnect and release the electrical harness grommet from the liftgate outer panel.
2. Release the center retention clip securing the applique to the liftgate outer panel.
3. Remove the liftgate applique.
4. Transfer parts as necessary.

## Liftgate Applique Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear window wiper motor. Refer to Rear Window Wiper Motor Replacement.

1 | Center Applique Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Center Applique Integral Clip

#### Procedure

Install the applique to the liftgate panel first by securing the integral clips.

3 | License Plate Lamp Electrical Connector

#### Procedure

Transfer the license plate lamp sockets and electrical harness to the new applique panel.

4 | Liftgate Center Applique