For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
2. Remove the remote battery ground stud.
3. Remove the underhood electrical center cover.
4. Reposition any wiring or hoses to gain access to air inlet screen.

1 | Air Inlet Screen

#### Procedure

1. Lift the air inlet grille panel enough to access the air inlet screen.
2. Use shop vacuum to remove any debris from the air inlet screen.