For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the wheelhouse liner in order to access the level indicator. Refer to Front Wheelhouse Front Liner Replacement.

1 | Windshield Washer Solvent Level Indicator

#### Procedure

1. Disconnect the electrical connector.
2. Using two flat-bladed tools under the lip of the level indicator, pry outward using a suitable clean container in order to recover the windshield washer solvent.
3. Discard the level indicator and grommet.