For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the headliner assembly. Refer to Headlining Trim Panel Replacement.

1 | Rear Seat Number 2 Center Seat Belt Retractor Assembly
2 | Rear Seat Number 2 Center Seat Belt Retractor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)