For 1990-2009 cars

## Side Window Defogger Outlet Grille Replacement - Right Side Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the right instrument panel air outlet assembly. Refer to Instrument Panel Outer Air Outlet Replacement - Right Side.

1 | Pal Nuts (Qty: 3)

#### Procedure

Tighten the pal nuts until fully seated but not stripped

2 | Side Window Defroster Outlet Duct Assembly
3 | Side Window Defroster Outlet Grille Assembly

## Side Window Defogger Outlet Grille Replacement - Right Side Enclave

Callout | Component Name
--- | ---
1 | Instrument Panel Trim Pad Refer to Instrument Panel Trim Pad Replacement.
2 | Instrument Panel Right Window Air Outlet Screw (Qty: 1) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Instrument Panel Right Window Air Outlet

#### Procedure

Release the tab on the air outlet from the underside of the trim pad and push the air outlet upward out of the trim pad.