For 1990-2009 cars

## Steering Column Housing Cover Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the steering wheel. Refer to Steering Wheel Replacement.
3. Remove the turn signal multifunction switch assembly. Refer to Turn Signal Multifunction Switch Replacement.
4. Remove the turn signal switch bracket. Refer to Turn Signal Switch Bracket Replacement.
5. Remove the instrument panel (I/P) cluster trim plate assembly. Refer to Instrument Panel Cluster Trim Plate Replacement.
6. Remove the instrument panel trim pad. Refer to Instrument Panel Trim Pad Replacement.
7. Remove the driver knee bolster. Refer to Driver Knee Bolster Replacement.

1 | Steering Column Housing Cover Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Steering Column Housing Cover Assembly

## Steering Column Housing Cover Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the steering wheel. Refer to Steering Wheel Replacement.
3. Remove the turn signal multifunction switch assembly. Refer to Turn Signal Multifunction Switch Replacement.
4. Remove the turn signal switch bracket. Refer to Turn Signal Switch Bracket Replacement.
5. Remove the instrument panel cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Replacement.
6. Remove the driver knee bolster assembly. Refer to Driver Knee Bolster Replacement.

1 | Steering Column Housing Cover Assembly Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Steering Column Housing Cover Assembly

## Steering Column Housing Cover Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the steering wheel. Refer to Steering Wheel Replacement.
3. Remove the turn signal multifunction switch assembly. Refer to Turn Signal Multifunction Switch Replacement.
4. Remove the turn signal switch bracket. Refer to Turn Signal Switch Bracket Replacement.
5. Remove the instrument panel cluster trim plate applique. Refer to Instrument Panel Cluster Trim Plate Applique Replacement.
6. Remove the driver knee bolster. Refer to Driver Knee Bolster Replacement.

1 | Steering Column Housing Cover Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Steering Column Housing Cover Assembly

## Steering Column Housing Cover Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the steering wheel. Refer to Steering Wheel Replacement.
3. Remove the turn signal multifunction switch assembly. Refer to Turn Signal Multifunction Switch Replacement.
4. Remove the turn signal switch bracket. Refer to Turn Signal Switch Bracket Replacement.
5. Remove the instrument panel cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Replacement.
6. Remove the knee bolster. Refer to Instrument Panel Compartment Replacement.

1 | Steering Column Housing Cover Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Steering Column Housing Cover Assembly