For 1990-2009 cars

### Removal Procedure

1. Remove the engine mount strut bracket. Refer to Engine Mount Strut Bracket Replacement - Right Side.
2. Remove the radiator inlet hose from the water outlet. Refer to Radiator Inlet Hose Replacement.
3. Remove the power steering fluid reservoir bracket bolts (1).
4. Remove and reposition the power steering fluid reservoir bracket (2) out of the way.
5. Disconnect the engine wiring harness electrical connector (8) from the bank 2 intake camshaft position (CMP) sensor (7).
6. Remove the CMP sensor bolt and sensor (3).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the CMP sensor (3) and bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

2. Connect the engine wiring harness electrical connector (8) to the bank 2 intake CMP sensor (7).
3. Position and install the power steering fluid reservoir bracket (2).
4. Install the power steering fluid reservoir bracket bolts (1).

Tighten
Tighten the bolts to 9 N·m (8 lb in).

5. Install the radiator inlet hose to the water outlet. Refer to Radiator Inlet Hose Replacement.
6. Install the engine mount strut bracket. Refer to Engine Mount Strut Bracket Replacement - Right Side.