For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the radiator inlet hose from the water outlet tube. Refer to Radiator Inlet Hose Replacement.
2. Remove the underhood fuse block bracket and fuse block. Refer to Underhood Electrical Center or Junction Block Replacement.

1 | Engine Mount Strut Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 58 N·m (43 lb ft)
2 | Engine Mount Strut