For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front floor console armrest compartment. Refer to Front Floor Console Armrest Compartment Replacement.

1 | Front Floor Console Armrest Latch Screw (Qty: 1) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5N·m(22 lb in)
2 | Front Floor Console Armrest Latch Assembly

#### Procedure

Ensure the rubber bumper on the end of the front floor console armrest latch is fully seated into the opening in the armrest assembly.