For 1990-2009 cars

## Three-Way Catalytic Converter Replacement With LLT

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Three Way Catalytiv Converter

#### Procedure

1. Disengage the hanger.
2. Remove and discard the gaskets.