For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.
3. Remove the outside door handle. Refer to Rear Side Door Outside Handle Replacement.

1 | Rear Side Door Outside Handle Housing Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Rear Side Door Lock Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
3 | Rear Side Door Outside Handle Housing

#### Procedures

1. Disconnect the lock and handle rods to remove the housing.
2. Release the inside handle cable retainers before removing the door lock.
3. Disconnect the door lock electrical connector.