For 1990-2009 cars

## Radiator Lower Grille Replacement Enclave

Callout | Component Name
--- | ---

#### Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the lower radiator retainers from the air baffle.

1 | Radiator Lower Grille Edge Type Clip (Qty: 15) Tip Release the clips from inside the lower radiator grille.
2 | Radiator Lower Grille Procedure Remove the lower grille from inside the lower bumper fascia.

## Radiator Lower Grille Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Radiator Lower Grille Tip Release the retainer tabs securing the lower radiator grille to the front bumper fascia opening.