For 1990-2009 cars

Checks | Causes
--- | ---
3-5-Reverse Clutch Assembly |

• | Inspect for improper surface finish on 3-5-Reverse Clutch Plates (423-426), Backing Plate (426)

• | Inspect for plugged or restricted oil passages and air bleed of the 3-5-Rev/4-5-6 Housing (422)

• | Inspect for damaged, worn or leaking 3-5-Reverse Clutch Piston Seals (419-421)

• | Inspect for warped 3-5-Rev/4-5-6 Clutch Housing (422)

• | Inspect for fatigued 3-5-Reverse Clutch Waved Plate (423)