For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the oil level indicator from the oil level indicator tube.
3. Remove the oil level indicator tube bolt.
4. Remove the oil level indicator tube up through the exhaust manifold.
5. If you are replacing only the oil level indicator tube seal, remove and discard the old seal.

### Installation Procedure

1. Install a new seal on the oil level indicator tube.
2. Install the oil level indicator tube.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the oil level indicator tube bolt and tighten to 10 N·m (89 lb in) .
4. Install the oil level indicator in the oil level indicator tube.