For 1990-2009 cars

Table 1: | Removal
Table 2: | Installation

### Removal

Callout | Component Name
--- | ---
1 | Front Differential Carrier Bearing Assembly

#### Special Tools

• | J-41816 Three Legged Puller

• | J 41816-2 Step Plate

For equivalent regional tools, refer to Special Tools.

2 | Inner Race Tip Ensure all 3 legs of the puller make contact with the inner race of the bearing.
3 | Front Differential Carrier Bearing Assembly Tip

• | AWD differential may need longer bolts, 2-3/8 x 5 x 24 thread bolts.

• | When removing the front differential carrier bearing assembly use J 41816-2 step plate .

#### Special Tools

• | J 8433-1 Puller Bar or equivalent

• | J 22912-B Split Plate Bearing Remover or equivalent

• | J 41816-2 Step Plate

For equivalent regional tools, refer to Special Tools.

### Installation

Callout | Component Name
--- | ---
1 | Front Differential Carrier Bearing Assembly Caution: Pressing against the bearing assembly can damage the bearing and cause premature bearing failure.

#### Special Tools

DT-47928 Bearing Installer

For equivalent regional tools, refer to Special Tools.

2 | Front Differential Carrier Bearing Assembly Caution: Pressing against the bearing assembly can damage the bearing and cause premature bearing failure.

#### Special Tools

DT-47928 Bearing Installer

For equivalent regional tools, refer to Special Tools.