For 1990-2009 cars

Checks | Causes
--- | ---
Case Assembly (51) |

• | Inspect for cracked or broken Case (51)

• | Inspect for stripped or sheared splines

• | Inspect for missing Lube Orifice Plug

• | Inspect for binding Manual Shift Detent Lever Assembly (511)

• | Inspect for missing Manual Shift Shaft Pin (510)

• | Inspect for interference or binding Park Pawl Actuator Assembly (509)

• | Inspect for disengaged or broken 1-2-3-4 Clutch Piston Spring Retainer (459)

Torque Converter |

• | Inspect for stripped or sheared splines on Turbine Shaft

• | Inspect for missing bolts from Torque Converter to Flywheel

35R/456 Housing Assembly |

• | Inspect for damaged or broken Input Shaft Thrust Bearing Assembly (32)

• | Inspect for stripped, sheared or loose splines on the Input Shaft to the 3-5 Reverse/4-5-6 Clutch Housing (422)

Oil Pump Assembly |

• | Inspect for fluid leaks / improper fluid level

• | Inspect for disengaged, worn, binding or failed Drive Sprocket (216), Driven Sprocket (215) or Drive Link (217)

• | Inspect for leaking Fluid Outlet Seal Assembly (57)

• | Inspect for damaged or worn Drive (219, 220) and Driven Sprocket Thrust Washers (214)

• | Inspect for loose or missing Oil Pump Bolts (204)

• | Inspect for stripped or sheared splines on the Oil Pump Shaft or Driven Sprocket (215)

• | Inspect for damaged, clogged or improperly installed Oil Filter Assembly (201)

• | Inspect for damaged or leaking Oil Filter Neck Seal (202)

Low & Reverse Clutch Assembly (455) | Inspect for stripped or sheared splines to the Reaction Carrier (467)
Input Carrier Assembly (470) |

• | Inspect for stripped or sheared splines to ring gear

• | Inspect for improperly installed carrier pinion gear pins