For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the fuel tank. Refer to Fuel Tank Replacement .
2. Remove the foam pad insulators.

1 | Fuel Tank
2 | Fuel Pump Fuel Feed Hose

#### Procedure

1. Disconnect the quick connect fitting from the module. Refer to Plastic Collar Quick Connect Fitting Service .
2. Disengage from the tank retaining features.
3. When installing, route under the evaporative emission (EVAP) canister vent front pipe.