For 1990-2009 cars

1. Install a NEW oil suction tube seal onto the oil suction tube. DO NOT reuse the old oil suction tube seal.
2. Install the oil suction pipe.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the oil suction pipe bolts and tighten to 10 N·m (89 lb in).
4. Install the oil pan scraper.
5. Install the oil pan scraper bolts and tighten to 10 N·m (89 lb in).
6. Install the oil pan drain plug and NEW O-ring seal and tighten the oil pan drain plug to 20 N·m (15 lb ft).