For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the bumper fascia. Refer to Rear Bumper Fascia Replacement.

1 | Rear Bumper Upper Fascia Rivet (Qty: 2) Warning: Approved safety glasses and gloves should be worn when performing this procedure to reduce the chance of personal injury.

#### Procedure

Drill out the rivets before removing the upper fascia.

2 | Rear Bumper Upper Fascia Tip Use a flat-bladed tool to release the tabs.