For 1990-2009 cars

## Daytime Running Lamp (DRL) Ambient Light Sensor Replacement Without UV6

Callout | Component Name
--- | ---
1 | Instrument Panel Upper Trim Panel Refer to Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement.
2 | Headlamp Auto Control Ambient Light Sensor Assembly

#### Procedure

1. Twist and pull down to remove.
2. Disconnect electrical connector.

## Daytime Running Lamp (DRL) Ambient Light Sensor Replacement With UV6

Callout | Component Name
--- | ---
1 | Instrument Panel Upper Trim Panel Refer to Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement.
2 | Headlamp Auto Control Ambient Light Sensor Assembly

#### Procedure

1. Twist and pull down to remove.
2. Disconnect electrical connector.