For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. It is only necessary to lower the headliner. Only do those step in headliner replacement that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement .
2. Remove the instrument upper trim panel. Refer to Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement .

1 | Sunroof Drain Hose Retainer (Qty: 2)
2 | Sunroof Drain Hose Coupler

#### Procedure

Disconnect the sunroof drain hose from the sunroof module spigot.

3 | Sunroof Drain Hose Plug
4 | Sunroof Drain Hose

#### Procedure

1. Installing the drain hose, ensure that the routing of the end of the drain hose is through the access hole in the cowl panel to prevent interior water leaks.
2. Install the 2 retainer that secure the drain hose to the windshield pillar.