For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat No. 2 assembly. Refer to Rear Number 2 Seat Replacement .

1 | Rear Seat No. 2 Cushion Cover

#### Procedure

1. Disconnect the j-channel from the seat cushion frame.
2. Remove the seat cushion cover and pad as an assembly from the frame.
3. Remove the seat cushion cover from the pad.

2 | Rear Seat No. 2 Cushion Pad