For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the coolant from the recovery reservoir.
2. Remove the front compartment sight shield if necessary. Refer to Front Compartment Sight Shields Replacement

1 | Coolant Recovery Reservoir Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Coolant Recovery Reservoir

#### Procedure

Remove overflow hose from reservoir