For 1990-2009 cars

## Rear Seat Back Cushion Cover and Pad Replacement with 40 Percent Seat without Armrest

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the rear seat latch release handle. Refer to Rear Seat Latch Release Handle Replacement .
3. Remove the rear seat latch release strap outer bezel. Refer to Rear Seat Latch Release Strap Bezel Replacement - Outer .
4. Remove the rear seat latch covers. Refer to Rear Seat Back Cushion Latch Cover Replacement - Inner or Rear Seat Back Cushion Latch Cover Replacement - Outer .
5. Remove the rear seat inner recliner cover. Refer to Rear Seat Recliner Inner Finish Cover Replacement - Upper .
6. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .
7. Remove the rear seat head restraint guides. Refer to Rear Seat Head Restraint Guide Replacement .

1 | Rear Seat Back Cushion Cover

#### Procedure

1. Unzip the seat cushion cover.
2. Disconnect the seat back cover j-channels from the seat back frame.
3. Remove the hog rings from the bottom of the seat back cover.
4. Remove the rear seat back cushion cover and pad as an assembly.

2 | Rear Seat Back Cushion Pad

#### Procedure

1. Disengage the hog rings retaining the cover to the pad.
2. Separate the seat back cushion cover from the pad.

## Rear Seat Back Cushion Cover and Pad Replacement with 40 Percent Seat with Armrest

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the rear seat latch covers. Refer to Rear Seat Back Cushion Latch Cover Replacement - Inner or Rear Seat Back Cushion Latch Cover Replacement - Outer .
3. Remove the rear seat latch release strap outer bezel.
4. Remove the rear seat armrest. Refer to Rear Seat Armrest Replacement .
5. Remove the rear seat inner recliner cover. Refer to Rear Seat Recliner Inner Finish Cover Replacement - Upper .
6. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .
7. Remove the rear seat head restraint guides. Refer to Rear Seat Head Restraint Guide Replacement .
8. Remove the rear seat armrest. Refer to Rear Seat Armrest Replacement .

1 | Rear Seat Back Cushion Cover

#### Procedure

1. Unzip the seat cushion cover.
2. Disconnect the seat back cover j-channels from the seat back frame.
3. Remove the hog rings from the bottom of the seat back cover.
4. Remove the rear seat back cushion cover and pad as an assembly.

2 | Rear Seat Back Cushion Pad

#### Procedure

1. Disengage the hog rings retaining the cover to the pad.
2. Separate the seat back cushion cover from the pad.

## Rear Seat Back Cushion Cover and Pad Replacement with 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the rear seat latch covers. Refer to Rear Seat Back Cushion Latch Cover Replacement - Inner or Rear Seat Back Cushion Latch Cover Replacement - Outer .
3. Remove the rear seat latch release strap outer bezel. Refer to Rear Seat Latch Release Strap Bezel Replacement - Outer .
4. Remove the rear seat latch release handle. Refer to Rear Seat Latch Release Handle Replacement .
5. Remove the rear seat armrest. Refer to Rear Seat Armrest Replacement .
6. Remove the rear seat inner recliner cover. Refer to Rear Seat Recliner Inner Finish Cover Replacement - Upper .
7. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .
8. Remove the rear seat head restraint guides. Refer to Rear Seat Head Restraint Guide Replacement .
9. Remove the rear seat shoulder belt opening bezel. Refer to Rear Seat Shoulder Belt Opening Bezel Replacement .

1 | Rear Seat Back Cushion Cover

#### Procedure

1. Unzip the seat cushion cover.
2. Disconnect the seat back cover j-channels from the seat back frame.
3. Remove the hog rings from the bottom of the seat back cover.
4. Remove the rear seat back cushion cover and pad as an assembly.

2 | Rear Seat Back Cushion Pad

#### Procedure

1. Disengage the hog rings retaining the cover to the pad.
2. Separate the seat back cushion cover from the pad.