For 1990-2009 cars

Checks | Causes
--- | ---
Torque Converter (27) | Inspect for damage.
Case Assembly (21) |

• | Inspect for porosity or damage on the sealing surfaces

• | Inspect for loose Oil Cooler Line Bolts or damaged Oil Cooler Line Seals

• | Inspect for damaged Manual Shift Shaft Seal (58)

• | Inspect for damaged or worn Axle Seal (61) or Axle Seal Slinger on the axle shafts

• | Inspect for loose Pressure Test Plug (62) and Fluid Level Plug (63)

Torque Converter Housing Assembly (221) |

• | Inspect for damaged Torque Converter Housing Assembly (25)

• | Inspect for porosity or damage on the sealing surfaces

• | Inspect for damaged Torque Converter Housing Seal (22)

• | Inspect for damaged or worn Torque Converter Fluid Seal (225)

• | Inspect for loose Torque Converter and Differential Housing Bolts (26)

• | Inspect for damaged or worn Axle Seal (226) or Axle Seal Slingers on the axle shafts

Case Cover assembly (34) |

• | Inspect for porosity or damage on the sealing surface

• | Inspect for damaged Case Cover Gasket (33)

• | Inpsect for loose Case Cover Assembly Bolts (35)

• | Inspect for loose Input Speed Sensor (ISS) Bolt (401)

• | Inspect for damaged Input Speed Sensor (ISS) Seal (402)

• | Inspect for loose, damaged or leaking Case Cover Assembly bore plugs

Valve Body Cover Assembly (1) |

• | Inpsect for damaged or warped Valve Body Cover Assembly (1)

• | Inspect for damaged Valve Body Cover Gasket (5)

• | Inspect for loose Valve Body Cover Bolts (7) and Valve Body Cover Studs (6)

• | Inspect for damaged or improperly installed Wire Connector Hole Seal (10)

• | Inspect for damaged or worn Fluid Level Indicator Seal

• | Inspect for plugged vent holes in the Fluid Level Indicator (2)