For 1990-2009 cars

## Automatic Transmission Shift Lock Control Actuator Replacement Acadia, Enclave, OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the front floor console extension panels. Refer to Front Floor Console Extension Panel Replacement - Right Side and Front Floor Console Extension Panel Replacement - Left Side.

1 | Shift Lock Actuator Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
2 | Shift Lock Actuator

#### Procedure

Shift lock actuator wires must be de-pinned from the electrical connector.

## Automatic Transmission Shift Lock Control Actuator Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front floor console extension panels. Refer to Front Floor Console Extension Panel Replacement - Right Side and Front Floor Console Extension Panel Replacement - Left Side.

1 | Shift Lock Actuator

#### Procedure

1. Disconnect the electrical connector from the shift lock actuator. Press lock on the solenoid wiring connector and remove by pulling on the connector, not the wire.
2. Depress the shift lock actuator retaining tabs and press the solenoid into the base by pushing on the solenoid housing, NOT the white plunger.
3. Connect the electrical connector from the shift lock actuator, ensuring the connector is fully locked into the solenoid.

Tip
Ensure the solenoid is fully locked into the base.