For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the ignition lock cylinder opening trim cover bolts. Refer to Ignition Lock Cylinder Opening Trim Cover Replacement.

1 | Steering Column Lower Trim Cover Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Steering Column Lower Trim Cover

#### Procedure

1. Unclip the steering column lower trim cover from the ignition lock cylinder opening trim cover.
2. Separate the steering column lower trim cover from the steering column upper trim cover.