For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the control valve lower body and upper body. Refer to Control Valve Lower Body and Upper Body Replacement.

1 | Output Speed Sensor Bolt M6 x 25 Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (106 lb in)
2 | Output Speed Sensor

#### Procedure

Perform the service fast learn adapt procedure. Refer to Service Fast Learn Adapts.

Tip
After an internal transmission repair or internal part replacement the service fast learn adapt procedure should be performed.