For 1990-2009 cars

# Service Stability Lamp DTC C0131- keywords ABS brake light message service stability

Subject: | Service Stability Lamp DTC C0131

Models: | 2007-2009 Buick Enclave

| 2007-2009 Cadillac Escalade, ESV, EXT

| 2007-2009 Chevrolet Avalanche, Silverado w/JL4, Suburban 1500, Tahoe

| 2007-2009 GMC Acadia, Sierra w/JL4, Yukon, Yukon Denali, Yukon XL 1500, Yukon Denali XL

| 2007-2009 Saturn Outlook

This PI was superceded to add 2009 model year and the Outlook, Acadia, Enclave. Please discard PIT4162C.

The following diagnosis might be helpful if the vehicle exhibits the symptom(s) described in this PI.

### Condition/Concern:

Some customers may comment of an ABS lamp illuminated followed by a Service Stability message displayed in the Drivers Information Center. After Initial diagnosis, technicians may find a diagnostic code C0131 set in the EBCM.

Removing an EBCM from one vehicle and installing it in another vehicle (for test purposes) will likely cause a DTC C0131 to set for a brake pressure sensor calibration value out of range. If this occurs, you will be unable to clear the DTC and the following procedure needs to be performed:

### Recommendation/Instructions:

If you experience this DTC after replacing the EBCM, perform a brake pressure sensor calibration with the Tech 2 by accessing the following menus:

Chassis/ EBCM/ Special Functions/ Brake Pressure Sensor Calibration.

Use the Tech 2 soft keys to "Enable" the calibration. After the soft key is pressed you should see the Command State change from "None" to "Enable". Continue to wait until the command state changes from "Enable" to "Off". Once completed, back out of the Tech 2 and turn off the Ignition Key and Tech 2 and wait 1 minute before cycling the key back on. This will allow the EBCM to complete the learn procedure.

Note: Make sure your Tech 2 is on the latest version. This reset function was not available until version 27.001, released 01/03/07.

Please follow this diagnostic or repair process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed.