For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left side catalytic converter. Refer to Catalytic Converter Replacement - Left Side
2. Support the engine. Refer to Engine Support Fixture.

1 | Front Engine Mount Upper Nut Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove and discard front engine mount upper nut.
2. Allow adhesive on new engine mount nuts to cure for 24 hours after replacement.

Tip

• | Use engine support fixture to raise engine.

• | The engine mount nuts must be replaced once removed.

Tighten
50 N·m (37 lb ft)

2 | Rear Engine Mount Upper Nut

#### Procedure

1. Remove and discard rear engine mount upper nut.
2. Allow adhesive on new engine mount nuts to cure for 24 hours after replacement.

Tip

• | Use engine support fixture to raise engine.

• | The engine mount nuts must be replaced once removed.

Tighten
50 N·m (37 lb ft)

3 | Front Engine Mount Bracket Bolt Tighten 58 N·m (43 lb ft)
4 | Front Engine Mount Bracket Tip To remove engine mount bracket, use engine support fixture to raise engine.