For 1990-2009 cars

#### Special Tools

J-28410 Gasket Remover

For equivalent regional tools, refer to Special Tools.

### Cleaning Procedure

1. Remove any RTV sealant (1) from the engine front cover using J-28410 remover .
2. Clean out debris from the bolt holes.
3. Clean the engine front cover in solvent.

Warning: Refer to Safety Glasses Warning in the Preface section.

4. Dry the engine front cover with compressed air.

### Inspection Procedure

1. Inspect the exterior of the engine front cover for the following conditions:

• | Damage to the camshaft position actuator valve oil seal bores (1)

• | Damage to the engine front cover bolt holes (2)

• | Damage and/or corrosion to the engine coolant passage (3)

• | Dents or damage to the exterior (4)

• | Damage to the crankshaft front oil seal bore (5)

• | Gouges or damage to the water pump sealing surfaces (6)

• | Damage to the water pump bolt hole threads (7)

2. Inspect the interior of the engine front cover for the following conditions:

• | Damage to the engine front cover bolt holes (1)

• | Gouges or damage to the engine front cover sealing surfaces to the engine block (7), oil pan (5), and/or camshaft covers (2)

• | Gouges or damage to the water pump seal area (3)

• | Loose or damaged deadener plates (4)

• | Damage and/or corrosion to the engine coolant passage (6)

• | Damage to the crankshaft front oil seal bore

• | Gouges or damage to the O-ring sealing areas

3. Repair or replace the engine front cover as necessary.