For 1990-2009 cars

### Removal Procedure

Note:

• | Always use replacement cables that are of the same type, diameter and length of the cables that you are replacing.

• | Always route the replacement cable the same way as the original cable.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the body wiring harness electrical connector (4) from the negative battery cable electrical connector (1).
3. Remove the negative battery cable ground bolt (2). (battery shown removed for clarity).
4. Remove the negative battery cable.

### Installation Procedure

1. Position the negative battery cable to the battery box. (battery shown removed for clarity).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the negative battery cable ground bolt (2).

Tighten
Tighten the bolt to 25 N·m (18 lb ft).

3. Connect the body wiring harness electrical connector (4) to the negative battery cable electrical connector (1).
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.