For 1990-2009 cars

### Removal Procedure

1. Remove the rear door sill plate. Refer to Rear Side Door Sill Plate Replacement .
2. Remove the weatherstrip (1) from the pinch-weld flange.

### Installation Procedure

1. Align the weatherstrip (1) to the door opening with the bond joint positioned at the lower center of the door opening.
2. Install the weatherstrip to the pinch-weld flange. Ensure the weatherstrip is fully seated.
3. Install the rear door sill plate. Refer to Rear Side Door Sill Plate Replacement .