For 1990-2009 cars

## Rear Window Wiper Blade Replacement GMC Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear wiper arm from the vehicle. Refer to Rear Window Wiper Arm Replacement.
2. Hold the arm stationary and rotate the blade in a vertical position.
3. Additional effort is required to push and install the wiper blade on and off from the wiper arm.

1 | Rear Window Wiper Blade Assembly Tip The wiper blade is fully secured to the wiper arm when an audible click noise is heard.

## Rear Window Wiper Blade Replacement Traverse

Callout | Component Name
--- | ---
1 | Rear Window Wiper Blade Assembly Tip Depress the tab under the wiper blade and pull the blade from the wiper arm sheep hook.