For 1990-2009 cars

## Door Lock Control Module Scan Tool Information Driver Door Switch

Table 1: | Driver Door Switch Scan Tool Data Parameters
Table 2: | Driver Door Switch Scan Tool Output Controls

#### Driver Door Switch Scan Tool Data Parameters

Parameter | System State | Expected Value | Definition
--- | --- | --- | ---
Operating Conditions: Ignition ON
Battery Voltage Signal | -- | Varies | This displays volts. This is the voltage input supplied to the driver door switch.
Door Key Cyl. Unlock Switch | -- | Idle | The scan tool displays Idle or Unlock. This is the state of the driver door key cylinder unlock switch.
Door Lock Actuator Cmd. | -- | Off | The scan tool displays Off, Unlock or Lock. This is the state of the door lock actuator.
Driver Door Ajar Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the driver door ajar switch.
Driver Door Open Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the driver door open switch.
Driver LF Window Switch | -- | Off | The scan tool displays Off, Up, Down, Express Up or Express Down. This is the state of the driver left front window switch.
Driver LR Window Switch | -- | Off | The scan tool displays Off, Up, Down, Express Up or Express Down. This is the state of the driver left rear window switch.
Driver RF Window Switch | -- | Off | The scan tool displays Off, Up, Down, Express Up or Express Down. This is the state of the driver right front window switch.
Driver RR Window Switch | -- | Off | The scan tool displays Off, Up, Down, Express Up or Express Down. This is the state of the driver right rear window switch.
Memory Recall Switches | -- | Varies | This displays volts. This is the voltage input supplied to the driver door memory recall switches.
Memory Switch 12V Ref. | -- | Varies | This displays volts. This is the voltage input supplied to the driver door memory switch.
Memory Switch Backlight | -- | Varies | The scan tool displays %. This is the intensity of the backlighting in the memory switch.
Mirror 5 Volt Reference | -- | ON | The scan tool displays On or Off. This is the state of the voltage reference circuit to the mirror.
Mirror Fold Switch | -- | Idle | The scan tool displays Idle, Extend or Retract. This is the state of the mirror fold switch.
Mirror Motor | -- | Idle | The scan tool displays Idle, Invalid, Up, Down, Left and Right. This is the state of the mirror motor.
Mirror Horizontal Position | -- | Varies | This displays volts. This is the voltage input supplied to the mirror horizontal position.
Mirror Select Switch | -- | Idle | The scan tool displays Idle, Right or Left. This is the state of the mirror select switch.
Mirror Vertical Position | -- | Varies | This displays volts. This is the voltage input supplied to the mirror vertical position.
Rear Window Sw. 12V Ref. | -- | Varies | This displays volts. This is the voltage input supplied to the rear window switch.
Seat Back Heat Mode Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat back heat mode indicator.
Seat Back Heat Mode Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the seat back heat mode switch.
Seat Cool Mode Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat cool mode indicator.
Seat Cool Mode Switch | -- | Off | The scan tool displays On or Off. This is the state of the seat cool mode switch.
Seat Heat High Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat high indicator.
Seat Heat Medium Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat medium indicator.
Seat Heat Low Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat low indicator.
Seat Heat Mode Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat mode.
Seat Heat Mode Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the seat heat mode switch.
VIN Learned | -- | Yes | The scan tool displays Yes or No. This is the state of the driver door switch VIN programming.
Window Lockout Switch | -- | Off | The scan tool displays On or Off. This is the state of the driver door window lockout switch.
Window Lockout Switch Indicator Command | -- | Off | The scan tool displays On or Off. This is the state of the driver door window lockout switch indicator.
Window Switch Backlight | -- | Varies | The scan tool displays %. This is the intensity of the backlighting in the window switch.

#### Driver Door Switch Scan Tool Output Controls

Scan Tool Output Control | Description
--- | ---
Door Deadbolt Lock/Unlock | This command will lock and unlock the driver door dead bolt actuator.
Door Lock/Unlock | This command will lock and unlock the driver door lock actuator.
Front Window Motor | This test will command the front window both up and down.
Heated Seat Indicators | This will command the heated seat indicators ON and OFF.
Integrated Sw. Backlighting Test | The scan tool commands the % intensity of the integrated switches backlighting.
Mirror Fold | This will command the driver mirror to fold and unfold.
Mirror Heater | This will command the driver mirror heater ON and OFF.
Mirror Left/Right | This will command the driver mirror left and right.
Mirror Up/Down | This will command the driver mirror up and down.
Non-Integrated Sw. Backlighting Test | The scan tool commands the % intensity of the non-integrated switches backlighting.
Power Window Motor Programming | This will enable the driver power window motor to be programmed.
Puddle/Courtesy Lamp | This will command the courtesy lamps ON and OFF.
Window Lockout Indicator | This will command the window lockout indicator ON and OFF.

## Door Lock Control Module Scan Tool Information Passenger Door Switch

Table 1: | Passenger Door Switch Scan Tool Data Parameters
Table 2: | Passenger Door Switch Scan Tool Output Controls

#### Passenger Door Switch Scan Tool Data Parameters

Parameter | System State | Expected Value | Definition
--- | --- | --- | ---
Operating Conditions: Ignition ON
Battery Voltage Signal | -- | Varies | This displays volts. This is the voltage input supplied to the passenger door switch.
Door Key Cyl. Unlock Switch | -- | Idle | The scan tool displays Idle or Unlock. This is the state of the passenger door key cylinder unlock switch.
Door Lock Actuator Cmd. | -- | Off | The scan tool displays Off, Unlock or Lock. This is the state of the door lock actuator.
Memory Switch 12V Ref. | -- | Varies | This displays volts. This is the voltage input supplied to the passenger door memory switch.
Memory Switch Backlight | -- | Varies | The scan tool displays %. This is the intensity of the backlighting in the memory switch.
Mirror 5-Volt Reference | -- | ON | The scan tool displays On or Off. This is the state of the voltage reference circuit to the mirror.
Mirror Horizontal Position | -- | Varies | This displays volts. This is the voltage input supplied to the mirror horizontal position.
Mirror Vertical Position | -- | Varies | This displays volts. This is the voltage input supplied to the mirror vertical position.
Passenger Door Ajar Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the passenger door ajar switch.
Passenger Door Open Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the passenger door open switch.
Passenger Window Switch | -- | Off | The scan tool displays Off, Up, Down, Express Up or Express Down. This is the state of the driver left front window switch.
Rear Window Sw. 12V Ref. | -- | Varies | This displays volts. This is the voltage input supplied to the rear window switch.
Seat Back Heat Mode Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat back heat mode indicator.
Seat Back Heat Mode Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the seat back heat mode switch.
Seat Cool Mode Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat cool mode indicator.
Seat Cool Mode Switch | -- | Off | The scan tool displays On or Off. This is the state of the seat cool mode switch.
Seat Heat High Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat high indicator.
Seat Heat Medium Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat medium indicator.
Seat Heat Low Ind. Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat low indicator.
Seat Heat Mode Cmd. | -- | Off | The scan tool displays On or Off. This is the state of the seat heat mode.
Seat Heat Mode Sw. | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the seat heat mode switch.
VIN Learned | -- | Yes | The scan tool displays Yes or No. This is the state of the passenger door switch VIN programming.
Window Switch Backlight | -- | Varies | The scan tool displays %. This is the intensity of the backlighting in the window switch.

#### Passenger Door Switch Scan Tool Output Controls

Scan Tool Output Control | Description
--- | ---
Door Deadbolt Lock/Unlock | This command will lock and unlock the passenger door dead bolt actuator.
Door Lock/Unlock | This command will lock and unlock the passenger door lock actuator.
Front Window Motor | This test will command the front window both Up and Down.
Heated Seat Indicators | This will command the heated seat indicators ON and OFF.
Integrated Sw. Backlighting Test | The scan tool commands the % intensity of the integrated switches backlighting.
Mirror Fold | This will command the passenger mirror to fold and unfold.
Mirror Heater | This will command the passenger mirror heater ON and OFF.
Mirror Left/Right | This will command the passenger mirror left and right.
Mirror Up/Down | This will command the passenger mirror up and down.
Non-Integrated Sw. Backlighting Test | The scan tool commands the % intensity of the non-integrated switches backlighting.
Power Window Motor Programming | This will enable the driver power window motor to be programmed.
Puddle/Courtesy Lamp | This will command the courtesy lamps ON and OFF.