For 1990-2009 cars

## Rear Window Washer Pump Replacement Acadia and Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the LF wheelhouse liner in order to access the washer pumps. Refer to Front Wheelhouse Front Liner Replacement.
2. Drain the washer solvent into a clean suitable container.
3. Disconnect the electrical connector.
4. Disconnect the washer pump hose.

1 | Rear Window Washer Pump Assembly

#### Procedure

1. Using two flat-bladed tools, at the pump gasket, pry upwards until the washer pump is disengaged from the windshield washer container.
2. Discard the washer pump grommet.

## Rear Window Washer Pump Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the LF wheelhouse liner in order to access the washer pumps. Refer to Front Wheelhouse Front Liner Replacement.
2. Drain the washer solvent into a clean suitable container.
3. Disconnect the electrical connector.

1 | Rear Window Washer Pump Assembly

#### Procedure

1. Using two flat-bladed tools, at the pump gasket, pry upwards until the washer pump is disengaged from the windshield washer container.
2. Discard the washer pump grommet.