For 1990-2009 cars

## Radiator Grille Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Radiator Grille Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Radiator Grille Assembly Tip Release the outer grille retainer tabs from the front bumper fascia and push outward in order to remove the grille.

## Radiator Grille Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front compartment sight shield. Refer to Front Compartment Sight Shields Replacement.

1 | Radiator Grille Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radiator Grille Assembly

#### Procedure

Release the 12 integral tabs using a small flat-bladed tool securing the radiator grille to the front bumper fascia.

## Radiator Grille Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the hood in order to access the fasteners for the radiator grille.

1 | Radiator Grille Support Bracket Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radiator Grille Support Bracket (Qty: 2)
3 | Radiator Grille Outer Bracket Bolt (Qty: 2) Tighten 2.5 N·m (22 lb in)
4 | Radiator Grille Upper Nut (Qty: 4) Tighten 9 N·m (80 lb in)
5 | Radiator Grille Assembly Tip Transfer the radiator grille emblem. Refer to Radiator Grille Emblem/Nameplate Replacement.