For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the body lock pillar upper garnish molding. Refer to Body Lock Pillar Upper Trim Panel Replacement.
3. Remove the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.

1 | Rear Seat Shoulder Belt Guide Adjuster Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Rear Seat Shoulder Belt Retractor Bolt Tighten 45 N·m (33 lb ft)
3 | Rear Seat Shoulder Belt Anchor Bolt Tighten 45 N·m (33 lb ft)
4 | Rear Seat Shoulder Belt Retractor Assembly