For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Following the deployment of a side impact air bag, inspect the following parts for damage. Replace these parts if necessary:

• | The seat cushion frame

• | The seat recliner, if equipped

• | The seat adjuster

• | The seat back frame

Failure to do so may cause future personal injury.

#### Preliminary Procedure

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the seat back cushion cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.

1 | Side Impact Inflatable Restraint Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Inflatable Restraint Module Assembly

#### Procedure

1. Unclip the side impact module wiring harness from under the seat.
2. Disconnect the electrical connector.
3. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping.
4. When replacing the inflatable restraint module, ensure the wire is secured inboard of the recline mechanism by utilizing the seat trim hook.