For 1990-2009 cars

#### Special Tools

• | EN 46106 Engine Flywheel Holding Tool

• | J 45059 Angle Meter

| For equivalent regional tools, refer to Special Tools.

1. Place the engine flywheel in position on the crankshaft.
2. Install 2 NEW bolts in location at the top and bottom of the engine flywheel bolt pattern allowing the engine flywheel to hang in position.
3. Install the EN 46106 tool .

Caution: Refer to Fastener Caution in the Preface section.

4. Install the remaining NEW engine flywheel bolts.

4.1. | Tighten the NEW engine flywheel bolts to 30 N·m (22 lb ft).

4.2. | Tighten the NEW engine flywheel bolts an additional 45 degrees using the J 45059 meter .

5. Remove the EN 46106 tool .