For 1990-2009 cars

## Radiator Grille Emblem/Nameplate Replacement Enclave

Callout | Component Name
--- | ---
1 | Radiator Grille Emblem (Tri-Shield)

#### Procedure

1. Open the hood.
2. Squeeze the 4 tabs on the emblem in order to unlock the emblem from the radiator grille.
3. Rotate the emblem in a counter-clockwise direction and push outward.
4. Remove the emblem from the radiator grille.

## Radiator Grille Emblem/Nameplate Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front radiator grille. Refer to Radiator Grille Replacement.

1 | Emblem Assembly (GMC) Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section. Procedure

1. Release the 4 retaining clips as heating the front radiator grille emblem.
2. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
3. Use a J 25070 Heat Gun or equivalent to remove the old nameplate. Clean all adhesive from grille and wipe the surface dry with a clean lint-free towel prior to installing the new name plate.
4. When removing protective liners from the adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
5. Align the two pins and 4 retaining clips into the grille opening.
6. Using the palm of the hand, wet out the emblem to the grille and ensure full adhesion of the emblem is made.