For 1990-2009 cars

Checks | Causes
--- | ---
3-5-Reverse Clutch Assembly |

• | Inspect for damaged, worn or stripped splines on 3-5-Reverse Clutch Plates (423-426), Backing Plate (426)

• | Inspect for sheared or stripped splines on 3-5-Rev/4-5-6 Housing to Turbine Shaft (422)

• | Inspect for damage, improper surface finish, porosity, deformed or unbalanced 3-5-Rev/4-5-6 Housing (422)

• | Inspect for damaged, worn, loose or seized hub bushing in the 3-5-Rev/4-5-6 Housing

• | Inspect for broken, porous or improper surface finish or plugged oil passages of the 3-5-Rev/4-5-6 Housing (422)

• | Inspect for failure of the Input Shaft Thrust Bearing (32)

• | Inspect for disengaged or broken 3-5-Reverse Clutch Backing Plate Retainer (427)

• | Inspect for damaged, worn or leaking 3-5-Reverse Clutch Piston Seals (419-421)

• | Inspect for damaged or broken 3-5-Rev/4-5-6 Clutch Housing (422)

• | Inspect for warped, damaged, improper surface finish or debonding 3-5-Reverse Clutch Piston (417)

• | Inspect for broken or fatigued 3-5-Reverse Clutch Spring (418)

• | Inspect for disengaged or broken Speed Sensor Reluctor Retainer (415)

• | Inspect for broken Speed Sensor Reluctor Wheel (416)

• | Inspect for seized Input Shaft Thrust Bearing (32)

Reaction Carrier (467) |

• | Inspect for broken or disengaged Input Internal Gear Retainer

• | Inspect for stripped or sheared splines on the Input Internal Gear

Output Carrier (474) | Inspect for stripped or sheared splines for the Reaction Internal Ring Gear
4-5-6 Clutch Assembly |

• | Inspect for plugged or missing 4-5-6 Piston Dam Oil Feed hole

• | Inspect for leaking 4-5-6 Piston Dam