For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear storage compartment. Refer to Rear Storage Compartment Replacement. (If equipped)

1 | Rear Seat No. 2 Assembly Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Rear Seat No. 2 Assembly (Qty: 2) Tip Lift the seat upward at the rear of the seat and slide the seat rearward to disengage the adjuster hooks holding the seat to the floor pan.