For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console filler. Refer to Front Floor Console Filler Replacement.
2. Remove the front floor console extension accessory upper bezel. Refer to Front Floor Console Extension Accessory Upper Bezel Replacement.

1 | Front Floor Console Armrest Assembly with Supports Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Floor Console Armrest Assembly with Supports