For 1990-2009 cars

Name | 6T70/6T75
--- | ---
RPO Codes | MH2, MH4 / MY9, MH6
Production Location | Warren Michigan (USA)
Transaxle Drive | Front Wheel Drive, All Wheel Drive
Reverse Gear Ratio | 2.88
1st Gear Ratio | 4.484
2nd Gear Ratio | 2.872
3rd Gear Ratio | 1.842
4th Gear Ratio | 1.414
5th Gear Ratio | 1.000
6th Gear Ratio | 0.742
Effective Final Drive Gear Ratio | 2.77/3.16
Torque Converter Size - Diameter of Torque Converter Turbine | 246 mm
Pressure Taps | Line Pressure
Transaxle Fluid Type | DEXRON VI®
Transaxle Fluid Capacity | 9.0 L/9.5 qts Quarts
Transaxle Type: 6 | Six Forward Gears
Transaxle Type: T | Transverse Mount
Transaxle Type: 70/75 | Product Series
Position Quadrant | P, R, N, D, * *(Refer to the applicable owner's manual)
Case Material | Die Cast Aluminum
Transaxle Net Weight | 104 kg
Maximum Trailer Towing Capacity | N/A
Maximum Gross Vehicle Weight (GVW) | 4,000 lbs